

# Asus RT-AC88U @ openWrt





#### Reset usine

1. Éteignez le routeur.
2. Appuyez et maintenez le bouton "WPS" puis allumez le routeur.
3. Le voyant d'alimentation est allumé **(continue à tenir le bouton WPS****).**
4. Relâchez le **bouton WPS** lorsque le voyant d'alimentation commence à clignoter.
5. Le voyant d'alimentation cesse de clignoter et le routeur redémarre automatiquement.

https://www.asus.com/fr/support/FAQ/1039077

Login / password: admin / admin





#### Copier le firmware sur le routeur:

Désactiver le coupe-feu de macOS.

```bash
~/Downloads                                                                                                                                   3m 59s 18:21:52
❯ tftp 192.168.1.1
tftp> mode binary
tftp> put openwrt-23.05.2-bcm53xx-generic-asus_rt-ac88u-squashfs.trx
Sent 9568256 bytes in 28.7 seconds

```



#### Connexion à OpenWrt:

```bash
root@192.168.1.1's password:


BusyBox v1.36.1 (2023-11-14 13:38:11 UTC) built-in shell (ash)

  _______                     ________        __
 |       |.-----.-----.-----.|  |  |  |.----.|  |_
 |   -   ||  _  |  -__|     ||  |  |  ||   _||   _|
 |_______||   __|_____|__|__||________||__|  |____|
          |__| W I R E L E S S   F R E E D O M
 -----------------------------------------------------
 OpenWrt 23.05.2, r23630-842932a63d
 -----------------------------------------------------
```



#### opkg

```bash
root@OpenWrt:~# opkg update
Downloading https://downloads.openwrt.org/releases/23.05.2/targets/bcm53xx/generic/packages/Packages.gz
Updated list of available packages in /var/opkg-lists/openwrt_core

root@OpenWrt:~# opkg find '*nano*'
nano - 7.2-2 - Nano is a small and simple text editor for use on the terminal.

root@OpenWrt:~# opkg install nano
Installing nano (7.2-2) to root...
```



#### Mise-à-jour

```bash
# opkg update && opkg install brcmfmac-firmware-4366b1-pcie
```



#### Infos

```bash
# uname -a
Linux OpenWrt 5.15.137 #0 SMP Tue Nov 14 13:38:11 2023 armv7l GNU/Linux
```

```bash
# cat /etc/os-release
NAME="OpenWrt"
VERSION="23.05.2"
ID="openwrt"
ID_LIKE="lede openwrt"
PRETTY_NAME="OpenWrt 23.05.2"
VERSION_ID="23.05.2"
HOME_URL="https://openwrt.org/"
BUG_URL="https://bugs.openwrt.org/"
SUPPORT_URL="https://forum.openwrt.org/"
BUILD_ID="r23630-842932a63d"
OPENWRT_BOARD="bcm53xx/generic"
OPENWRT_ARCH="arm_cortex-a9"
OPENWRT_TAINTS=""
OPENWRT_DEVICE_MANUFACTURER="OpenWrt"
OPENWRT_DEVICE_MANUFACTURER_URL="https://openwrt.org/"
OPENWRT_DEVICE_PRODUCT="Generic"
OPENWRT_DEVICE_REVISION="v0"
OPENWRT_RELEASE="OpenWrt 23.05.2 r23630-842932a63d"
```

```bash
# cat /proc/cpuinfo
processor	: 0
model name	: ARMv7 Processor rev 0 (v7l)
BogoMIPS	: 1400.00
Features	: half thumb fastmult edsp tls
CPU implementer	: 0x41
CPU architecture: 7
CPU variant	: 0x3
CPU part	: 0xc09
CPU revision	: 0

processor	: 1
model name	: ARMv7 Processor rev 0 (v7l)
BogoMIPS	: 1400.00
Features	: half thumb fastmult edsp tls
CPU implementer	: 0x41
CPU architecture: 7
CPU variant	: 0x3
CPU part	: 0xc09
CPU revision	: 0

Hardware	: BCM5301X
Revision	: 0000
Serial		: 0000000000000000
```



### Liens



#### OpenWrt:

- [Table of Hardware](https://openwrt.org/toh/start)
- [Table of Hardware: devices with 16/128MB or more](https://openwrt.org/toh/views/toh_available_16128)
- 
- [OpenWrt Support for Asus RT-AC88U](https://forum.openwrt.org/t/openwrt-support-for-asus-rt-ac88u/78635)

- [OpenWrt Wiki](https://openwrt.org/toh/asus/rt-ac88u)

- [Quick start guide for OpenWrt installation](https://openwrt.org/docs/guide-quick-start/start)

- [OpenWrt Factory Install](https://openwrt.org/docs/guide-quick-start/factory_installation)

#### Firmwares:

- [OpenWrt Firmware Selector](https://firmware-selector.openwrt.org/?version=23.05.2&target=bcm53xx%2Fgeneric&id=asus_rt-ac88u) -

-  [Archive Firmwares](https://archive.openwrt.org/releases/23.05.2/targets/bcm53xx/generic/)

#### TFTP:

- [Installing openWrt via TFTP](https://openwrt.org/docs/guide-user/installation/generic.flashing.tftp)
- [Setting up a TFTP server for TFTP Recovery/Install](https://openwrt.org/docs/guide-user/troubleshooting/tftpserver)
- [Run a TFTP Server for Network Device Setups](https://rick.cogley.info/post/run-a-tftp-server-on-mac-osx/)
- [TFTP Server for macOS](https://macandegg.com/2022/02/tftp-server-for-macos/)



#### Livebox:

- [[La fibre.info] Remplacement de la Livebox par un routeur Openwrt](https://lafibre.info/remplacer-livebox/remplacement-de-la-livebox-par-un-routeur-openwrt-18-dhcp-v4v6-tv/)

- [[Github] Remplacer une Livebox par un routeur OpenWrt (ipv4,ipv6 & TV)](https://github.com/ubune/openwrt-livebox)

- [[La fibre.info] Index des solutions de remplacement de la Livebox](https://lafibre.info/remplacer-livebox/index-des-solutions-de-remplacement-de-la-livebox/)



#### Divers:

- [SNBForums (Asus)](https://www.snbforums.com/forums/asus-wireless.37/)
- [[La fibre.info] OpenWrt](https://lafibre.info/openwrt/)
